set $CLIENT_BUMBLEBEE -m disk nic sensors battery caffeine amixer brightness datetime -p battery.device=BAT0,BAT1 brightness.device_path=/sys/class/backlight/acpi_video0 disk.format={left} nic.states=^down sensors.path=/sys/class/thermal/thermal_zone2/temp  -t greyish-powerline


# {{{ VARIABLES  }}}

    set $mod Mod4
    set $TERMINAL urxvt

    # gaps
    set $gap_outer 25
    set $gap_inner 15

    set $ws1 "1 "
    # Terminal
    set $ws2 "2 "
    # Work
    set $ws3 "3 "
    set $ws4 "4"
    # Mail
    set $ws5 "5 "
    set $ws6 "6"
    set $ws7 "7"
    set $ws8 "8"
    set $ws9 "9"
    set $ws10 "10"
